List of figures

Figure 1.1 Major dams (greater than 500 GL capacity), large irrigation areas and selected drainage divisions across Australia 3

Figure 1.2 Schematic diagram of key components and concepts in the establishment of a greenfield irrigation development 7

Figure 2.1 The Flinders and Gilbert catchments within the Gulf region of northern Australia 10

Figure 2.2 The Flinders catchment 11

Figure 2.3 Soil sampling sites and airborne geophysical survey flight lines of the Flinders catchment 14

Figure 2.4 Schematic representation of digital soil mapping method 15

Figure 2.5 Availability of rainfall data in the Flinders catchment 16

Figure 2.6 Crop yield (rice) and applied irrigation water 27

Figure 3.1 Schematic diagram of key natural components and concepts in the establishment of a greenfield irrigation development 34

Figure 3.2 Simplified surface geology of the Flinders catchment 37

Figure 3.3 Soil generic group (SGG) classes for the Flinders catchment 40

Figure 3.4 Surface soil pH of the Flinders catchment 42

Figure 3.5 Minimum soil depth of the Flinders catchment 42

Figure 3.6 Soil surface texture of the Flinders catchment 43

Figure 3.7 Soil permeability of the Flinders catchment 44

Figure 3.8 Plant available water capacity in the Flinders catchment 45

Figure 3.9 Electrical conductivity in soils of the Flinders catchment 46

Figure 3.10 Typical synoptic systems influencing the Flinders catchment 47

Figure 3.11 Mean annual rainfall and mean annual potential evaporation under Scenario A 48

Figure 3.12 Rainfall under Scenario A for the Flinders catchment 49

Figure 3.13 Potential evaporation under Scenario A for the Flinders catchment 49

Figure 3.14 Rainfall deficit under Scenario A for the Flinders catchment 49

Figure 3.15 Rainfall and potential evaporation under Scenario A averaged across the Flinders catchment 50

Figure 3.16 Mean annual rainfall and potential evaporation under Scenario A averaged over the Flinders catchment 51

Figure 3.17 Rainfall variability around Australia under Scenario A 52

Figure 3.18 Runs of wet and dry years in the Flinders catchment under Scenario A 53

Figure 3.19 Percentage change in mean annual rainfall and potential evaporation under Scenario C relative to Scenario A 54

Figure 3.20 Spatial distribution of mean annual rainfall across the Flinders catchment under scenarios Cwet, Cmid and Cdry 55

Figure 3.21 Mean monthly rainfall and potential evaporation for the Flinders catchment under scenarios A and C 55

Figure 3.22 Schematic diagram of terrestrial water balance in the Flinders catchment 56

Figure 3.23 Major aquifers of the Flinders catchment 57

Figure 3.24 Schematic cross-section highlighting the connectivity between aquifers of the Carpentaria and Karumba basins of the Great Artesian Basin 58

Figure 3.25 Groundwater salinity in the Flinders catchment with the recharge area of the Great Artesian Basin and the location of airborne electromagnetic flight lines shown in Figure 3.26 and Figure 3.27 59

Figure 3.26 Satellite image and conductivity-depth section for flight line 10325 60

Figure 3.27 Satellite image and conductivity-depth section for flight line 10211 62

Figure 3.28 Map of mean annual groundwater recharge in the Flinders catchment under Scenario A 63

Figure 3.29 Likelihood of groundwater inflow at river and waterhole sampling sites in the Flinders catchment 65

Figure 3.30 Main rivers and streamflow gauging stations of the Flinders catchment 66

Figure 3.31 Change in catchment area along the Flinders River from Glendower to Flinders river mouth 67

Figure 3.32 Change in catchment area along the Cloncurry River from Agate Downs to confluence with Flinders River 67

Figure 3.33 Mean annual rainfall and runoff across the Flinders catchment under Scenario A 68

Figure 3.34 Maps showing 20%, 50% and 80% exceedance annual runoff across the Flinders catchment under Scenario A 68

Figure 3.35 Runoff in the Flinders catchment under Scenario A 69

Figure 3.36 Cloncurry River upstream of Cloncurry (January 2013) 69

Figure 3.37 Median annual streamflow (i.e. 50% exceedance) in the Flinders catchment under Scenario A 72

Figure 3.38 20% and 80% exceedance of annual streamflow in the Flinders catchment under Scenario A 73

Figure 3.39 Flood inundation map of Flinders catchment 74

Figure 3.40 Comparative spatial extent and temporal variation of inundation 75

Figure 3.41 Instream waterhole evolution 76

Figure 3.42 Location of key aquatic refugia identified in the Flinders catchment. Inset shows river reaches investigated 77

Figure 4.1 Schematic diagram of key components of the living and built environment to be considered in the establishment of a greenfield irrigation development 82

Figure 4.2 Characteristics of the Flinders River 85

Figure 4.3 Extent of fish surveys in Flinders catchment 87

Figure 4.4 Saw-shelled turtle captured in the Gilbert catchment 88

Figure 4.5 Example of a typical turbid waterhole in the Flinders River 90

Figure 4.6 Status of regional ecosystem biodiversity status for the Flinders catchment 93

Figure 4.7 Spatial representation of important ecological assets across the Flinders catchment 94

Figure 4.8 Diagram of Indigenous dam from the Flinders area 96

Figure 4.9 Current native title determinations and applications in the Flinders catchment 98

Figure 4.10 Indigenous land use agreements and Indigenous-controlled pastoral leases in the Flinders catchment 99

Figure 4.11 Total live cattle export from Australia, September 1992 to September 2012 112

Figure 4.12 Current mining and mineral exploration and development leases in the Flinders catchment 114

Figure 4.13 Petroleum, geothermal and coal exploration licences and existing dams in the Flinders catchment 115

Figure 4.14 Chinaman Creek Dam looking upstream 117

Figure 4.15 Corella River Dam looking upstream 118

Figure 4.16 Multi-combination vehicles 119

Figure 4.17 Queensland infrastructure map showing accessibility of heavy vehicles, ports and railways in Queensland and the Flinders catchment 120

Figure 4.18 Flinders catchment infrastructure map showing accessibility of heavy vehicles, ports, railways and high voltage powerlines 121

Figure 5.1 Schematic diagram of key engineering and agricultural components to be considered in the establishment of a greenfield irrigation development 132

Figure 5.2 Schematic diagram of an embankment dam 135

Figure 5.3 DamSite model results for the Flinders catchment overlain on transparent geology and shaded relief map 138

Figure 5.4 Cost of water in $/ML versus cumulative divertible yield at 85% annual time reliability 143

Figure 5.5 Cave Hill dam site looking upstream 145

Figure 5.6 Dam cross-section, height, volume and reservoir surface area for Cave Hill dam site 145

Figure 5.7 Cave Hill Dam depth of inundation and property boundaries 146

Figure 5.8 Annual time reliability and volumetric reliability for Cave Hill dam under scenarios A and C 147

Figure 5.9 Comparisons of inundated area with and without the construction of Cave Hill dam under Scenario A 147

Figure 5.10 Regional ecosystems inundated by the potential Cave Hill dam reservoir at full supply level 148

Figure 5.11 A depiction of the O’Connell Creek offstream storage, looking upstream 149

Figure 5.12 Dam cross-section, height, volume and reservoir surface area for O’Connell Creek offstream storage 150

Figure 5.13 O’Connell Creek offstream storage depth of inundation and property boundaries 150

Figure 5.14 Annual time and volumetric reliability for O’Connell Creek offstream storage under scenarios A and C 151

Figure 5.15 Regional ecosystems inundated by the potential O’Connell Creek offstream storage at full supply level 152

Figure 5.16 Porcupine Creek dam site looking upstream 153

Figure 5.17 Dam cross-section, height, volume and reservoir surface area for Porcupine Creek potential dam site 153

Figure 5.18 Porcupine Creek dam depth of inundation 154

Figure 5.19 Annual time reliability and volumetric reliability for Porcupine Creek dam under scenarios A and C 155

Figure 5.20 Comparisons of inundated area with and without the construction of Porcupine Creek dam under Scenario A 155

Figure 5.21 Regional ecosystems inundated by the Porcupine Creek dam at full supply level 156

Figure 5.22 Schematic diagram of sheet piling weir 157

Figure 5.23 Rectangular ring tank 160

Figure 5.24 Annual volume of streamflow extracted versus annual time reliability for streamflow gauge 915204A 161

Figure 5.25 Annual volume of streamflow extracted versus annual time reliability for streamflow gauge 915008A 161

Figure 5.26 Annual volume of streamflow extracted versus annual time reliability for streamflow gauge 915003A 161

Figure 5.27 Land suitability for offstream water storages in the Flinders catchment 163

Figure 5.28 Reported conveyance losses from irrigation systems across Australia (ANCID, 2001) 168

Figure 5.29 Efficiency of different types of irrigation systems 169

Figure 5.30 Probability of crop yield potential for dryland and fully irrigated mungbean sown in Richmond climate on 15 January 179

Figure 5.31 Probability of yield potential for dryland and fully irrigated sorghum (grain) sown in Richmond climate on 15 January 179

Figure 5.32 Probability of yield potential for dryland and fully irrigated cotton sown in Richmond climate on 15 January 179

Figure 5.33 Crop yield plotted against applied irrigation water in Richmond climate 181

Figure 5.34 Applied irrigation water for planting on the 15th day of each month for sorghum (grain) at Richmond 186

Figure 5.35 Crop yield for planting on the 15th day of each month for sorghum (grain) at Richmond 187

Figure 5.36 The area associated with each land suitability class for a selection of 13 crops in the Flinders catchment 190

Figure 5.37 Modelled land suitability for sorghum (grain). Note that this land suitability map does not take into consideration flooding, risk of secondary salinisation or availability of water 192

Figure 5.38 Sorghum (grain) 192

Figure 5.39 Modelled land suitability for mungbean. Note that this land suitability map does not take into consideration flooding, risk of secondary salinisation or availability of water 195

Figure 5.40 Mungbean 195

Figure 5.41 Modelled land suitability for Rhodes grass and sorghum (forage). Note that this land suitability map does not take into consideration flooding, risk of secondary salinisation or availability of water 199

Figure 5.42 Bambatsi 199

Figure 5.43 Modelled land suitability for lablab and lucerne. Note that this land suitability map does not take into consideration flooding, risk of secondary salinisation or availability of water 202

Figure 5.44 Lablab 202

Figure 5.45 Modelled land suitability for cotton. Note that this land suitability map does not take into consideration flooding, risk of secondary salinisation or availability of water 206

Figure 5.46 Cotton 206

Figure 5.47 Modelled land suitability for sugarcane. Note that this land suitability map does not take into consideration flooding, risk of secondary salinisation or availability of water 209

Figure 5.48 Sugarcane 209

Figure 5.49 Modelled land suitability for sweet corn and tomato. Note that this land suitability map does not take into consideration flooding, risk of secondary salinisation or availability of water 212

Figure 5.50 Sweet corn 212

Figure 5.51 Modelled land suitability for mango and Indian sandalwood. Note that this land suitability map does not take into consideration flooding, risk of secondary salinisation or availability of water 215

Figure 5.52 Indian sandalwood 215

Figure 5.53 Modelled land suitability for mango and Indian sandalwood. Note that this land suitability map does not take into consideration flooding, risk of secondary salinisation or availability of water 219

Figure 5.54 Mangoes 219

Figure 6.1 Schematic diagram of key components and concepts in the establishment of a greenfield irrigation development 228

Figure 6.2 Growth patterns of beef cattle in northern Australia 231

Figure 6.3 Land tenure in the Flinders catchment 252

Figure 7.1 Schematic diagram of key components and concepts in the establishment of a greenfield irrigation development 256

Figure 7.2 Steady-state watertable level for (a) various recharge rates and hydraulic conductivities (K) and (b) an irrigation area of 100 ha, at varying distances to the river 261

Figure 7.3 Steady-state watertable level for an irrigation area of 1000 ha, plotted against distance to the river 261

Figure 7.4 Steady-state watertable level at varying distances to the river for an irrigation area of (a) 250 ha and (b) 500 ha 262

Figure 7.5 Steady-state watertable level at varying distances (d) to the river for (a) an irrigation area of 1000 ha and (b) various irrigation area and distance combinations 262

Figure 7.6 Watertable level for various aquifer diffusivities (D) and distances to river (d), for an irrigation area of 100 ha and recharge rate of 100 mm/year 263

Figure 7.7 Flux response for different aquifer diffusivities, for different hydraulic conductivities (K), specify yields (Sy) and distances to river (d) 263

Figure 7.8 Variation in watertable level beneath two neighbouring 500-ha irrigation developments at different distances of separation 264

Figure 7.9 Conductivity–depth section (lower panel) for flight line 10230. Location of flight line on a satellite image is shown in upper panel. This flight line transects the Flinders River downstream of Hughenden 265

Figure 8.1 Schematic diagram illustrating the components of the case study for an irrigation development near Cloncurry, with feedlot, abattoir and Cave Hill dam 277

Figure 8.2 (a) Satellite map and (b) relief map of the area surrounding Cave Hill dam 280

Figure 8.3 (a) Soil generic group map and (b) land suitability map of the area surrounding Cave Hill dam for spray-irrigated sorghum (grain) 282

Figure 8.4 Landscape of the potential Cave Hill dam irrigation development, facing east 283

Figure 8.5 (a) Monthly rainfall and (b) monthly potential evaporation, under Scenario A at Cloncurry 284

Figure 8.6 (a) Maximum monthly temperature and (b) minimum monthly temperature, under Scenario A at Cloncurry 284

Figure 8.7 Annual streamflow at the Cave Hill dam site under Scenario A 285

Figure 8.8 Crop yield versus applied irrigation water under Scenario A for sorghum (grain) in the Cloncurry area 290

Figure 8.9 Mean annual applied irrigation water supplied to the field in (a) ML and (b) ML/ha under Scenario B for the irrigation development associated with the Cave Hill dam 292

Figure 8.10 (a) Median annual applied irrigation water supplied to the field and (b) percentage of years that the maximum area is planted under Scenario B for the irrigation development associated with the Cave Hill dam 292

Figure 8.11 Ratio of evaporation from the reservoir to the applied irrigation water under Scenario B for the irrigation development associated with the Cave Hill dam 293

Figure 8.12 (a) Percentage of time the volume of the reservoir is less than dead storage volume and (b) percentage of time the volume of the reservoir is less than 20% of the full supply level volume under Scenario B for the irrigation development associated with the Cave Hill dam 293

Figure 8.13 Mean annual streamflow quotient at (a) gauge 915203A and (b) gauge 915003A for the irrigation development associated with the Cave Hill dam 294

Figure 8.14 (a) Median of the 30-year mean values (M30M) for crop yield and (b) standard deviation of the 30-year mean values (S30M) for crop yield under Scenario B for the irrigation development associated with the Cave Hill dam 295

Figure 8.15 Annual crop yield from the irrigation development under Scenario B for three different scheme areas 295

Figure 8.16 (a) Median of the 30-year mean values (M30M) for specific yield and (b) percentage of time 82,500 t of grain is exceeded under Scenario B for the irrigation development associated with the Cave Hill dam 296

Figure 8.17 (a) Median of the 30-year mean values (M30M) for gross margin and (b) median of the 30-year mean values for gross margin per hectare under Scenario B for the irrigation development associated with the Cave Hill dam 297

Figure 8.18 (a) Median of the 30-year net present values and (b) standard deviation of the 30-year net present values under Scenario B for the irrigation development associated with the Cave Hill dam 298

Figure 8.19 (a) Median of the 30-year net present values and (b) standard deviation of the 30-year net present values under Scenario B for the irrigation development associated with the Cave Hill dam 299

Figure 8.20 Gross margins for sorghum (grain) under Scenario B for the irrigation development associated with the Cave Hill dam, with a scheme area of 12,000 ha and crop area decision of 4 ML/ha: (a) time series and (b) box plot 300

Figure 8.21 Percentage exceedance plots of (a) net present value and (b) internal rate of return under Scenario B for the scheme-scale irrigation development of 12,000 ha associated with the Cave Hill dam 301

Figure 8.22 Percentage exceedance plots of net present value under Scenario B for the farm-scale irrigation development of 12,000 ha associated with the Cave Hill dam 302

Figure 8.23 Change in depth to watertable for different values of saturated hydraulic conductivity (K): (a) low recharge rate of 67 mm/year and (b) high recharge rate of 118 mm/year 303

Figure 9.1 Schematic diagram illustrating the components of the case study for an irrigation development near Maxwelton, with O’Connell Creek offstream storage 309

Figure 9.2 (a) Satellite map and (b) relief map of the area surrounding O’Connell Creek offstream storage 311

Figure 9.3 (a) Soil generic group map and (b) land suitability map for the O’Connell Creek offstream storage and Maxwelton area for sugarcane (spray irrigation) 313

Figure 9.4 Landscape at Maxwelton looking south 314

Figure 9.5 Conductivity–depth section (lower panel) for flight line 10,490 (see Figure 9.2), and location of flight line on a satellite image (upper panel) 315

Figure 9.6 Conductivity–depth section (lower panel) for flight line 10,690 (see Figure 9.2), and location of flight line on a satellite image (upper panel) 315

Figure 9.7 (a) Monthly rainfall and (b) potential evaporation under Scenario A at Richmond 316

Figure 9.8 (a) Maximum monthly temperature and (b) minimum monthly temperature, Scenario A at Richmond 317

Figure 9.9 Annual streamflow at the O’Connell Creek offstream storage under Scenario A 318

Figure 9.10 Crop yield versus irrigation water under Scenario A for rice in the Maxwelton area 322

Figure 9.11 Mean annual applied irrigation water supplied to the field in (a) ML and (b) ML/ha under Scenario B for the irrigation development associated with the O’Connell Creek offstream storage 324

Figure 9.12 (a) Median annual applied irrigation water supplied to the field and (b) percentage of years that the maximum area is planted under Scenario B for the irrigation development associated with the O’Connell Creek offstream storage 324

Figure 9.13 (a) Ratio of evaporation from the reservoir to the applied irrigation water and (b) percentage of time the volume of the reservoir is less than 20% of the full supply level volume under Scenario B for the irrigation development associated with the O’Connell Creek offstream storage 325

Figure 9.14 Median annual streamflow quotient at (a) dummy gauge 943 and (b) gauge 915003A for the irrigation development associated with the O’Connell Creek offstream storage. Virtual gauge 943 is a node created within the Source river model 325

Figure 9.15 (a) Median of the 30-year mean values (M30M) for crop yield and (b) standard deviation of the 30-year mean values (S30M) for crop yield under Scenario B for the irrigation development associated with the O’Connell Creek offstream storage 326

Figure 9.16 Crop yield from the total scheme area under Scenario B for three different scheme areas. Lines correspond to circles show in Figure 9.15 327

Figure 9.17 (a) Median of the 30-year mean values (M30M) for specific yield and (b) percentage of time 50,000 t of grain is exceeded under Scenario B for the irrigation development associated with the O’Connell Creek offstream storage 327

Figure 9.18 (a) Median of the 30-year mean values (M30M) for gross margin per hectare and (b) median of the 30-year mean values (M30M) for gross margin under Scenario B, for the irrigation development associated with the O’Connell Creek offstream storage 329

Figure 9.19 (a) Median of the 30-year mean values (M30M) for net present value and (b) standard deviation of the 30-year mean values (S30M) for net present value under Scenario B for the irrigation development associated with the O’Connell Creek offstream storage 330

Figure 9.20 (a) Median of the 30-year mean values (M30M) for net present value and (b) standard deviation of the 30-year mean values (S30M) for net present value under Scenario B for the irrigation development associated with the O’Connell Creek offstream storage 331

Figure 9.21 Gross margins for rice under Scenario B for the 5300-ha irrigation development associated with the O’Connell Creek offstream storage 332

Figure 9.22 Percentage exceedance plots for the scheme-scale analysis of (a) net present value and (b) internal rate of return under Scenario B for the 5300-ha irrigation development associated with the O’Connell Creek offstream storage 333

Figure 9.23 Percentage exceedance plots for the farm-scale analysis of (a) net present value and (b) internal rate of return under Scenario B for the 5300-ha irrigation development associated with the O’Connell Creek offstream storage 334

Figure 9.24 Change in depth to watertable for different values of saturated hydraulic conductivity (K) 335

Figure 10.1 Schematic diagram illustrating the components of the case study for the water harvesting irrigation development in the Flinders catchment 341

Figure 10.2 (a) Relief and broad-scale flood inundation map and (b) offstream water storage suitability map of the Flinders catchment 344

Figure 10.3 (a) Soil generic group map and (b) land suitability map of surface-irrigated cotton in the Flinders catchment 346

Figure 10.4 Area associated with each land suitability class for a selection of 13 crops in the Flinders catchment, excluding land inundated by flooding 347

Figure 10.5 Area associated with each land suitability class for a selection of 13 crops in the Flinders catchment, excluding land underlain by the Rolling Downs Group (Figure 10.3b) 348

Figure 10.6 Area associated with each land suitability class for a selection of 13 crops in the Flinders catchment, excluding land inundated by flooding, underlain by the Rolling Downs Group (Figure 10.3b) or more than 5 km from a river of catchment area greater than 250 km2 348

Figure 10.7 (a) Monthly rainfall and (b) monthly potential evaporation at Richmond under Scenario A 349

Figure 10.8 (a) Monthly maximum temperature and (b) monthly minimum temperature at Richmond under Scenario A 349

Figure 10.9 Reliability of extracting water up to the annual entitlement for ten irrigators for three ‘storage size to entitlement-to-pump capacity’ (SSEPC) ratios (5, 10 and 20) by 1 February under Scenario B320 354

Figure 10.10 Reliability of extracting water up to the annual entitlement for ten water harvesting users for three ‘storage size to entitlement-to-pump capacity’ (SSEPC) ratios (5, 10 and 20) by 1 July under Scenario B320 355

Figure 10.11 Reliability of extracting water up to the entitlement for ten water harvesting users by 1 January under Scenario B. Assuming a ‘storage size to entitlement-to-pump capacity’ (SSEPC) ratio of 5 357

Figure 10.12 Reliability of extracting water up to the entitlement for ten water harvesting users by 1 February under Scenario B. Assuming a ‘storage size to entitlement-to-pump capacity’ (SSEPC) ratio of 5 358

Figure 10.13 Reliability of extracting water up to the entitlement for ten water harvesting users by 1 July under Scenario B. Assuming a ‘storage size to entitlement-to-pump capacity’ (SSEPC) ratio of 5 359